Q1. - Does the supplier have any liabilities for the technological process?

- No, the supplier is responsible for supply, delivery, unloading, installation and commissioning of the machines.

 Q2. – Is the Seed cleaning machine intended for the primary or final cleaning of the seeds?

 - The Seed cleaning machine will be used for the final cleaning before the pressing.

 Q3. - Does the technical specification of seed capacity of the flaxseed oil pressing machine refer to input or output capacity?

 - To the input capacity.

 Q4. – Should the prices be offered for each item separately?

- Yes, the financial offer should be presented as a breakdown, although the offers received will be compared in total values.

 Q5. – Are the production areas ready for installation of the equipment?

 - Yes, the production areas are renovated and furnished with all necessary systems.

 Q6. – Is it possible to fix the contract prices and pay in EUR?

 - No, according to the legislation of RA the payment currency in Armenia is AMD.

 Q7. – Do the contract foresee a pre-payment?

- For the 50% pre-financing the pre-financing guarantee should be submitted (Article 26.5, of the Special conditions).

Q8. – Should we offer only the prices of the machinery?

- The financial offers should include all costs related to the delivery, installation and commissioning.

Q9. – Do the contract also envision the training of the staff?

- No, the contract does not suppose training.

Q11. - Should we submit the bank guarantee in the tender documents or after the contract signature?

- The pre-financing guarantee will be requested after the contract signature.

Q12. - How much is the level of the precision of the Digital floor weighting scale (150kg)

- 50-100gr

Q13. - The display of the Digital floor weighting scales should be on the stand or attached to the platform?

- The display should be on the stand.

Q14. - How much is the length of the cable of the display?

- 2-3 m.

Q15. – Should the scales be with or without the weights for internal calibration?

- With.

Q16. -Is there a need for external weights for calibration (if there are no internal)?

- Yes.

Q17. - For which external conditions (explosive, dry storage, increased moisture, washable areas.) are the scales intended?

- The scales are intended for dry storages.

Q18. - For which grains are the Screw loaders intended? (Lot 1)

- Spelt, wheat, barley, spelt groats.

Q19. - What is the angle of inclination of Screw loaders? (Lot 1)

- N/A. It depends on the length of the pipe.

Q20. – What is the needed productivity of the Screw loaders? (Lot 1)

- 1.8-2.2 t/h.

Q21. - What length is needed along the axes of the nozzles?

- 3.5-4m.